.encoding = "windows-1252"
config.version = "8"
virtualHW.version = "10"
scsi0.present = "TRUE"
scsi0.virtualDev = "lsilogic"
memsize = "128"
ethernet0.present = "TRUE"
ethernet0.wakeOnPcktRcv = "FALSE"
ethernet0.addressType = "generated"
pciBridge0.present = "TRUE"
pciBridge4.present = "TRUE"
pciBridge4.virtualDev = "pcieRootPort"
pciBridge4.functions = "8"
pciBridge5.present = "TRUE"
pciBridge5.virtualDev = "pcieRootPort"
pciBridge5.functions = "8"
pciBridge6.present = "TRUE"
pciBridge6.virtualDev = "pcieRootPort"
pciBridge6.functions = "8"
pciBridge7.present = "TRUE"
pciBridge7.virtualDev = "pcieRootPort"
pciBridge7.functions = "8"
vmci0.present = "TRUE"
hpet0.present = "TRUE"
usb.vbluetooth.startConnected = "TRUE"
displayName = "DD-WRT v24"
guestOS = "debian5"
nvram = "DD-WRT v24.nvram"
virtualHW.productCompatibility = "hosted"
powerType.powerOff = "soft"
powerType.powerOn = "soft"
powerType.suspend = "soft"
powerType.reset = "soft"
extendedConfigFile = "DD-WRT v24.vmxf"
uuid.bios = "56 4d f3 8f 35 3f 1d af-01 04 bc f9 fc fa 90 5f"
uuid.location = "56 4d ab c6 95 48 b1 cc-9c cd 7a 60 05 75 f7 a7"
replay.supported = "FALSE"
replay.filename = ""
pciBridge0.pciSlotNumber = "17"
pciBridge4.pciSlotNumber = "21"
pciBridge5.pciSlotNumber = "22"
pciBridge6.pciSlotNumber = "23"
pciBridge7.pciSlotNumber = "24"
scsi0.pciSlotNumber = "16"
ethernet0.pciSlotNumber = "32"
vmci0.pciSlotNumber = "33"
ethernet0.generatedAddress = "00:0c:29:fa:90:5f"
ethernet0.generatedAddressOffset = "0"
vmci0.id = "-50687905"
monitor.phys_bits_used = "40"
vmotion.checkpointFBSize = "33554432"
cleanShutdown = "TRUE"
softPowerOff = "FALSE"
ide0:0.present = "TRUE"
ide0:0.fileName = "hdd0.vmdk"
ide0:0.redo = ""
bios.forceSetupOnce = "FALSE"
tools.remindInstall = "TRUE"
ide1:0.present = "FALSE"
ide0:1.present = "FALSE"
ide1:1.present = "FALSE"
floppy0.present = "FALSE"
